# Digital Offshore Cadastre (DOC) - Pacific83 - Official Protraction Diagram (OPD) Outlines Clipped

Metadata also available as

# Metadata:

- Identification_Information
- Data_Quality_Information
- Spatial_Data_Organization_Information
- Spatial_Reference_Information
- Entity_and_Attribute_Information
- Distribution_Information
- Metadata_Reference_Information

Identification_Information:
  Citation:
    Citation_Information:
      Originator: Bureau of Ocean Energy Management, Mapping and Boundary Branch
      Publication_Date: 20060210
      Title:
        Digital Offshore Cadastre (DOC) - Pacific83 - Official Protraction Diagram (OPD) Outlines Clipped
      Geospatial_Data_Presentation_Form: Map
      Series_Information:
        Series_Name: Digital Offshore Cadastre
        Issue_Identification: current
      Publication_Information:
        Publication_Place: Herndon, Virginia
        Publisher: Bureau of Ocean Energy Management, Mapping and Boundary Branch
      Online_Linkage:
        <http://www.boem.gov/Oil-and-Gas-Energy-Program/Mapping-and-Data/Pacific-files/protclip.zip>
      Online_Linkage:
        <http://www.boem.gov/Oil-and-Gas-Energy-Program/Mapping-and-Data/Pacific.aspx>
      Larger_Work_Citation:
        Citation_Information:
          Originator: Bureau of Ocean Energy Management, Mapping and Boundary Branch
          Publication_Date: 200205
          Title:
            Technical Information Management System (TIMS), Mapping System, Block and Boundary Component
          Geospatial_Data_Presentation_Form: Map
          Publication_Information:
            Publication_Place: Herndon, Virginia
            Publisher:
              Bureau of Ocean Energy Management, Mapping and Boundary Branch
  Description:
    Abstract:
      This data set contains Official Protraction Diagram (OPD) outlines in ESRI Arc/Info export and Arc/View shape file formats for the BOEM Pacific Region. The use of OPD s makes it easier to refer to individual blocks within a region or planning area. Further information on the historic development of OPD s can be found in OCS Report BOEM 99-0006: Boundary Development on the Outer Continental Shelf. These OPD diagrams were clipped along the Submerged Lands Act (SLA) boundary and along lines contained in the Continental Shelf Boundaries (CSB) GIS data files to show only those blocks or portions thereof within federal jurisdiction. Because GIS projection and topology functions can change or generalize coordinates, these GIS files are NOT an OFFICIAL record for the exact OPD boundaries. Only the paper OPD or a digital image of them serve as OFFICIAL records.
    Purpose:
      Official Protraction Diagrams and other cadastre information the BOEM produces are generated in accordance with 30 Code of Federal Regulations (CFR) 256.8 to support Federal land ownership and mineral resource management.
    Supplemental_Information:
      The BOEM is making its existing cadastre data available at <http://www.boem.gov/Oil-and-Gas-Energy-Program/Mapping-and-Data/Index.aspx> and on CD-ROM. These data will include digital images of BOEM data at the regional, planning area, Official Protraction Diagram (OPD), and Supplemental Official OCS Block Diagram (SOBD) levels and digital spatial data in Arc/Info export or Arc/View shape format at the regional or planning area levels.
  Time_Period_of_Content:
    Time_Period_Information:
      Single_Date/Time:
        Calendar_Date: 200205
    Currentness_Reference: Publication date
  Status:
    Progress: Complete
    Maintenance_and_Update_Frequency: As needed
  Spatial_Domain:
    Bounding_Coordinates:
      West_Bounding_Coordinate: -130.26
      East_Bounding_Coordinate: -117.18
      North_Bounding_Coordinate: 48.51
      South_Bounding_Coordinate: 30.10
  Keywords:
    Theme:
      Theme_Keyword_Thesaurus: None
      Theme_Keyword: Offshore
      Theme_Keyword: Cadastre
      Theme_Keyword: Official Protraction Diagram, OPD
      Theme_Keyword: Lease blocks
      Theme_Keyword: Outer Continental Shelf, OCS
      Theme_Keyword: OCS blocks
      Theme_Keyword: Bureau of Ocean Energy Management, BOEM
      Theme_Keyword: Oil and gas
    Place:
      Place_Keyword_Thesaurus: None
      Place_Keyword: USA
      Place_Keyword: Pacific Ocean
      Place_Keyword: Exclusive Economic Zone, EEZ
      Place_Keyword: California, CA
      Place_Keyword: Oregon, OR
      Place_Keyword: Washington, WA
  Access_Constraints:
    None. The Block and Boundary data is in the public domain.
  Use_Constraints:
    The data was developed within the U.S. Government; no proprietary rights may be attached to them nor may they be sold to the U.S. Government as part of any procurement of ADP products or services.
  Point_of_Contact:
    Contact_Information:
      Contact_Organization_Primary:
        Contact_Organization:
          Bureau of Ocean Energy Management, Mapping and Boundary Branch
        Contact_Person: Branch Chief, Mapping and Boundary Branch
      Contact_Position: Branch Chief
      Contact_Address:
        Address_Type: Mailing address
        Address: 381 Elden Street
        City: Herndon
        State_or_Province: Virginia
        Postal_Code: 20170
        Country: USA
      Contact_Voice_Telephone: (703) 787-1312
      Contact_Facsimile_Telephone: (703) 787-1236
      Contact_Electronic_Mail_Address:
      Contact_Electronic_Mail_Address: mapping.boundary.branch@BOEM.gov
      Hours_of_Service: 8:00am-6:00pm ET
  Browse_Graphic:
    Browse_Graphic_File_Name: pac_prot.gif
    Browse_Graphic_File_Description:
      An image of the BOEM Pacific Region Official Protraction Diagram (OPD) Outlines GIS data file.
    Browse_Graphic_File_Type: GIF
  Native_Data_Set_Environment:
    Coverages were created in Arc/Info version 7.0.4 on a Sun Sparc Station 10 running Solaris 2.5.1
  Cross_Reference:
    Citation_Information:
      Originator: Bureau of Ocean Energy Management, Mapping and Boundary Branch
      Publication_Date: 1997-2002
      Title: Supplemental Official OCS Block Diagrams (SOBD s)
      Edition: current version
      Geospatial_Data_Presentation_Form: Diagram
      Publication_Information:
        Publication_Place: Herndon, Virginia
        Publisher: Bureau of Ocean Energy Management, Mapping and Boundary Branch
      Other_Citation_Details:
        SOBD s contain additional coordinate and area calculations for individual blocks.
      Online_Linkage:
        <http://www.boem.gov/Oil-and-Gas-Energy-Program/Mapping-and-Data/Index.aspx>
      Larger_Work_Citation:
        Citation_Information:
          Originator: Bureau of Ocean Energy Management, Mapping and Boundary Branch
          Publication_Date: 200111
          Title:
            Technical Information Management System (TIMS), Mapping System, Block and Boundary Component
  Cross_Reference:
    Citation_Information:
      Originator:
        Bureau of Ocean Energy Management, Pacific Region, Leasing Activities Section
      Publication_Date: Unpublished material
      Title: Leases
      Publication_Information:
        Publication_Place: Camarillo, California
        Publisher:
          Bureau of Ocean Energy Management, Pacific Region, Leasing Activities Section
      Other_Citation_Details:
        This Oracle database contains current information on the status of Federal leases.
      Larger_Work_Citation:
        Citation_Information:
          Originator: Bureau of Ocean Energy Management
          Publication_Date: 2002
          Title:
            Technical Information Management System (TIMS), Lease Administration Component

Data_Quality_Information:
  Logical_Consistency_Report:
    Coordinates for OCS blocks and projected boundaries are calculated quantities and have been defined to be correct to 3 decimal places of a meter. The OPD polygon coverage was topologically cleaned with Arc/Info s CLEAN command using a fuzzy tolerance of 0.000002 applied to the coverage in longitude/latitude coordinates.
  Completeness_Report:
    All NAD83 Federal Pacific Ocean offshore protraction diagram (OPD) boundaries are shown.
  Positional_Accuracy:
    Horizontal_Positional_Accuracy:
      Horizontal_Positional_Accuracy_Report:
        Official protraction diagram (OPD) corners are calculated values to 3 decimal places of a meter. However, GIS functions which build topology, change projection, etc. may degrade coordinate values. For that reason, these GIS files are NOT an OFFICIAL record.
  Lineage:
    Source_Information:
      Source_Citation:
        Citation_Information:
          Originator: Bureau of Ocean Energy Management, Mapping and Boundary Branch
          Publication_Date: 2002
          Title: TIMS, Mapping Syetem, Block and Boundary Component
          Geospatial_Data_Presentation_Form: Map
          Publication_Information:
            Publication_Place: Herndon, Virginia
            Publisher:
              Bureau of Ocean Energy Management, Mapping and Boundary Branch
      Type_of_Source_Media: Computer program
      Source_Time_Period_of_Content:
        Time_Period_Information:
          Single_Date/Time:
            Calendar_Date: 2002
        Source_Currentness_Reference: Publication date
      Source_Citation_Abbreviation: BOEM, TIMS
      Source_Contribution:
        Coordinates of the protraction diagram corners were taken from TIMS.
    Process_Step:
      Process_Description:
        The source data for the OCS protraction diagram coverage (OPD) is a theoretical mathematical derivation. In-house computer programs are used to generate the boundaries for each diagram. These OPD diagrams were clipped along the Submerged Lands Act (SLA) boundary and along lines contained in the Continental Shelf Boundaries (CSB) GIS data files to show only those blocks or portions thereof within federal jurisdiction.
      Source_Used_Citation_Abbreviation: BOEM, TIMS
      Process_Date: 20020625
      Process_Contact:
        Contact_Information:
          Contact_Organization_Primary:
            Contact_Organization:
              Bureau of Ocean Energy Management, Mapping and Boundary Branch
            Contact_Person:
          Contact_Position: Branch Chief
          Contact_Address:
            Address_Type: Mailing address
            Address: 381 Elden Street
            City: Herndon
            State_or_Province: Virginia
            Postal_Code: 20170
            Country: USA
          Contact_Voice_Telephone: (703) 787-1312
          Contact_Facsimile_Telephone: (703) 787-1236
          Contact_Electronic_Mail_Address:
          Contact_Electronic_Mail_Address: mapping.boundary.branch@BOEM.gov
          Hours_of_Service: 8:00am-6:00pm ET

Spatial_Data_Organization_Information:
  Indirect_Spatial_Reference: U.S. Pacific Outer Continental Shelf (OCS)
  Direct_Spatial_Reference_Method: Vector
  Point_and_Vector_Object_Information:

Spatial_Reference_Information:
  Horizontal_Coordinate_System_Definition:
    Geographic:
      Latitude_Resolution: 0.00000001
      Longitude_Resolution: 0.00000001
      Geographic_Coordinate_Units: Decimal degrees
    Geodetic_Model:
      Horizontal_Datum_Name: North American Datum 1983
      Ellipsoid_Name: Geodetic Reference System 80
      Semi-major_Axis: 6378137 m
      Denominator_of_Flattening_Ratio: 298.25722210088

Entity_and_Attribute_Information:
  Detailed_Description:
    Entity_Type:
      Entity_Type_Label: PC_PROT_CLIP
    Attribute:
      Attribute_Label: FID
      Attribute_Definition: Internal feature number.
      Attribute_Definition_Source: ESRI
      Attribute_Domain_Values:
        Unrepresentable_Domain:
          Sequential unique whole numbers that are automatically generated.
    Attribute:
      Attribute_Label: Shape
      Attribute_Definition: Feature geometry.
      Attribute_Definition_Source: ESRI
      Attribute_Domain_Values:
        Unrepresentable_Domain: Coordinates defining the features.
    Attribute:
      Attribute_Label: OBJECTID
    Attribute:
      Attribute_Label: PROT_NUMBE
    Attribute:
      Attribute_Label: PROT_APRV_
    Attribute:
      Attribute_Label: AREA_CODE
    Attribute:
      Attribute_Label: MMS_REGION
    Attribute:
      Attribute_Label: Shape_Leng
    Attribute:
      Attribute_Label: Shape_Area
      Attribute_Definition: Area of feature in internal units squared.
      Attribute_Definition_Source: ESRI
      Attribute_Domain_Values:
        Unrepresentable_Domain: Positive real numbers that are automatically generated.
    Attribute:
      Attribute_Label: PROT_NAME
    Attribute:
      Attribute_Label: PROJ_ZONE_
    Attribute:
      Attribute_Label: DATUM_CODE
    Attribute:
      Attribute_Label: PLAN_CODE
    Attribute:
      Attribute_Label: PLAN_NAME
  Overview_Description:
    Entity_and_Attribute_Overview:
      The shape files contain the following entities: Shape: Polygon Area: Size of polygon in ESRI coverage units Perimeter: Perimeter of polygon in ESRI coverage units Protrac_: Internal ESRI number Protrac_id: Internal ESRI number BOEM_region: BOEM region code (P = Pacific) Prot_numbe: BOEM OPD identification number Prot_aprv: BOEM OPD approval date (day-month-year) Prot_name: BOEM OPD/map name Proj_zone: OPD UTM map projection zone code (9 = 132W to 126W longitude, 10 = 126W to 120W longitude, 11 = 120W to 114W longitude)
    Entity_and_Attribute_Detail_Citation: Bureau of Ocean Energy Management

Distribution_Information:
  Distributor:
    Contact_Information:
      Contact_Organization_Primary:
        Contact_Organization:
          Bureau of Ocean Energy Management, Mapping and Boundary Branch
      Contact_Address:
        Address_Type: Mailing address
        Address: 381 Elden Street
        City: Herndon
        State_or_Province: Virginia
        Postal_Code: 20170
        Country: USA
      Contact_Voice_Telephone: (703) 787-1312
      Contact_Facsimile_Telephone: (703) 787-1236
      Contact_Electronic_Mail_Address: mapping.boundary.branch@BOEM.gov
      Hours_of_Service: 8:00am-6:00pm ET
  Resource_Description: Digital Offshore Cadastre
  Distribution_Liability:
    As is. No responsibility is assumed for the correctness of this data.
  Standard_Order_Process:
    Digital_Form:
      Digital_Transfer_Information:
        Format_Name: ARCE
        Format_Version_Number: 7.0.4
        Transfer_Size: 1.9 Mbytes
      Digital_Transfer_Option:
        Online_Option:
          Computer_Contact_Information:
            Network_Address:
              Network_Resource_Name:
                <http://www.boem.gov/Oil-and-Gas-Energy-Program/Mapping-and-Data/Index.aspx>
          Access_Instructions:
            From the GIS Coverages section of the website html page, click on the Arc/Info .e00 Export file you wish to download. The downloaded file will need to be uncompressed. In a UNIX environment use uncompress filename . In a DOS environment use gzip -d filename . The resulting file will be an Arc/Info export data file (filename.e00).
          Online_Computer_and_Operating_System:
            Dell Pentium server running Windows NT 4.0
    Digital_Form:
      Digital_Transfer_Information:
        Format_Name: ASHP
        Format_Version_Number: 3
        Transfer_Size: 2.0 Mbytes
      Digital_Transfer_Option:
        Online_Option:
          Computer_Contact_Information:
            Network_Address:
              Network_Resource_Name:
                <http://www.boem.gov/Oil-and-Gas-Energy-Program/Mapping-and-Data/Index.aspx>
          Access_Instructions:
            From the GIS Coverages section of the website html page, click on the Arc/View shapefile file you wish to download. The downloaded file will need to be unzipped. The result will be the necessary Arc/View shapefiles and .dbf file.
          Online_Computer_and_Operating_System:
            Dell Pentium server running Windows NT 4.0
    Fees: None

Metadata_Reference_Information:
  Metadata_Date: 20040624
  Metadata_Review_Date: 20040624
  Metadata_Contact:
    Contact_Information:
      Contact_Organization_Primary:
        Contact_Organization:
          Bureau of Ocean Energy Management, Mapping and Boundary Branch
        Contact_Person:
      Contact_Position: Branch Chief
      Contact_Address:
        Address_Type: Mailing address
        Address: 381 Elden Street
        City: Herndon
        State_or_Province: Virginia
        Postal_Code: 20170
        Country: USA
      Contact_Voice_Telephone: (703) 787-1312
      Contact_Facsimile_Telephone: (703) 787-1236
      Contact_Electronic_Mail_Address:
      Contact_Electronic_Mail_Address: mapping.boundary.branch@BOEM.gov
      Hours_of_Service: 8:00am - 6:00pm ET
  Metadata_Standard_Name: Content Standard for Digital Geospatial Metadata
  Metadata_Standard_Version: FGDC-STD-001-1998
  Metadata_Time_Convention: Local time

Generated by `mp` version 2.9.6 on Fri Aug 03 14:28:41 2012